**Crate Late Models**  
Fastrak. Nesmith, SECA rules apply. – 12” spoiler OK –   
  
Siping & Grooving OK (NO PREP)  
  
Approved Tires include  
American Racer Spec 48 and Spec 56  
  
Protests – $1000 to protest an engine – 70% goes to the winning driver – 30% goes to the Tech Official and promoter. If the driver, who protests, wants a certified rebuilder to look at the engine, it will be at the protester’s expense.  
  
2350 lbs weight limit; 50 lb weight break for containment seat or Hahns device.   
  
NOTE: Ford sealed engine 347sr legal in Crate Late Model 2016…tech by Ford engine manual.