**Crate Late Models**
Fastrak. Nesmith, SECA rules apply. – 12” spoiler OK –

Siping & Grooving OK (NO PREP)

Approved Tires include
American Racer Spec 48 and Spec 56

Protests – $1000 to protest an engine – 70% goes to the winning driver – 30% goes to the Tech Official and promoter. If the driver, who protests, wants a certified rebuilder to look at the engine, it will be at the protester’s expense.

2350 lbs weight limit; 50 lb weight break for containment seat or Hahns device.

NOTE: Ford sealed engine 347sr legal in Crate Late Model 2016…tech by Ford engine manual.